DTC DETECTION LOGIC NOTE：

- If DTC B2602 is displayed with DTC U1000, first perform the trouble diagnosis for DTC U1000. Refer to DTC Logic.
- If DTC B2602 is displayed with DTC U1010, first perform the trouble diagnosis for DTC U1010. Refer to DTC Logic.

DTC No. | Trouble diagnosis name | DTC detecting condition | Possible cause
B2602 | SHIFT POSITION | BCM detects the following status for 10 seconds.

- Shift position is in the P position
- Vehicle speed is 4 km/h (2.5 MPH) or more
- Ignition switch is in the ON position

- Harness or connectors
  (A/T shift selector circuit is open or shorted)
- A/T shift selector (detention switch)
- ABS actuator and electric unit (control unit)
- BCM

DTC CONFIRMATION PROCEDURE
1.PERFORM DTC CONFIRMATION PROCEDURE

1. Start the engine under the following conditions and wait for at least 10 seconds.

- Shift lever is in the P or N position.
- Depress the brake pedal.

2. Check “Self diagnostic result” with CONSULT-III.

Is DTC detected?
YES>>Go to Diagnosis Procedure.
NO>>INSPECTION END