1.CHECK PARKING LAMP FUSE

1. Turn the ignition switch OFF.
2. Check that the following fuse is not fusing.

Unit | Location | Fuse No. | Capacity
Parking lamp | IPDM E/R | #52 | 10 A

Is the fuse fusing?
YES>>GO TO 2.
NO>>GO TO 3.
2.CHECK PARKING LAMP SHORT CIRCUIT

1. Disconnect IPDM E/R connector and the front combination lamp connector.
2. Check continuity between the IPDM E/R harness connector and the ground.

   IPDM E/R | Ground | Continuity
   Connector | Terminal
   RH | E9 | 91 | Not existed
   LH | 92

Does continuity exist?
YES>>Repair the harnesses or connectors. And then replace the fuse.
NO>>Replace the fuse. (Replace IPDM E/R if fusing is found again.)
3.CHECK PARKING LAMP BULB
Check the applicable lamp bulb.
Is the bulb normal?
YES>>GO TO 4.
NO>>Replace the bulb.
4.CHECK PARKING LAMP OUTPUT VOLTAGE
CONSULT-III ACTIVE TEST

1. Disconnect the front combination lamp connector.
2. Turn the ignition switch ON.
3. Select "EXTERNAL LAMPS" of IPDM E/R active test item.
4. With operating the test items, check the voltage between the IPDM E/R harness connector and the ground.

   Terminals | Test item | Voltage (Approx.)
   (+) | (−)
   IPDM E/R | Ground | EXTERNAL LAMPS
   Connector | Terminal
   RH | E9 | 91 | TAIL | Battery voltage
   Off | 0 V
   LH | 92 | TAIL | Battery voltage
   Off | 0 V

Is the measurement value normal?
YES>>GO TO 5.
NO>>Replace IPDM E/R.
5.CHECK PARKING LAMP OPEN CIRCUIT

1. Turn the ignition switch OFF.
2. Disconnect the IPDM E/R connector.
3. Check continuity between the IPDM E/R harness connector and the front combination lamp harness connector.

   IPDM E/R | Front combination lamp | Continuity
   Connector | Terminal | Connector | Terminal
   RH | E9 | 91 | E28 | 8 | Existed
   LH | 92 | E58 | 8

Does continuity exist?
YES>>GO TO 6.
NO>>Repair the harnesses or connectors.
6.CHECK PARKING LAMP GROUND OPEN CIRCUIT
Check continuity between the front combination lamp harness connector and the ground.

Front combination lamp | Ground | Continuity
Connector | Terminal
RH | E28 | 4 | Existed
LH | E58 | 4

Does continuity exist?
YES>>Replace the front combination lamp.
NO>>Repair the harnesses or connectors.