The Intelligent Key has the same functions as the remote control entry system. Therefore, it can be used in the same manner as the remote controller by operating the door lock/unlock button. OPERATION Remote keyless entry system controls operation of the following items.

- Door lock/unlock
- Selective unlock
- Trunk open
- Hazard and horn reminder
- Auto door lock
- Panic alarm
- Interior lamp

OPERATION AREA
To check that the Intelligent Key works normally, use within 1 m (3 ft) range of each doors, however the operable range may differ according to surroundings.
DOOR LOCK/UNLOCK FUNCTION

- When door lock/unlock button of the Intelligent Key is pressed, lock signal or unlock signal transmitted from Intelligent Key to BCM via remote keyless entry receiver.
- When BCM receives the door lock/unlock signal, it operates all door lock actuators and fuel lid lock actuator the hazard lamp (lock: 2 times, unlock: 1 time) and horn chirp signal to IPDM E/R at the same time as a reminder.
- IPDM E/R honks horn (lock: 2 times) as a reminder

OPERATION CONDITION

Remote controller operation | Operation condition
Lock |

- More than 3 seconds are passed since intelligent Key is removed from key slot.
- Panic alarm is not activated
- P position warning is not activated

Unlock |

- More than 3 seconds are passed since intelligent Key is removed from key slot.
- Panic alarm is not activated

SELECTIVE UNLOCK FUNCTION

- When an LOCK signal is transmitted from Intelligent Key, all doors and fuel lid are locked.
- When an UNLOCK signal is transmitted from Intelligent Key once, driver side door and fuel lid are unlocked.
- Then, if an UNLOCK signal is transmitted from Intelligent Key again within 60 seconds, all other doors are unlocked.

Selective unlock operation mode can be changed using “DOOR LOCK-UNLOCK SET” mode in “WORK SUPPORT”. Refer to CONSULT-III Function (BCM - DOOR LOCK).
TRUNK OPEN FUNCTION

- When trunk button of the Intelligent Key is pressed, the trunk open signal is transmitted from the Intelligent Key to the BCM via remote keyless entry receiver.
- When BCM receives the trunk open request signal, it operates the trunk lid opener actuator and opens the trunk.

OPERATION CONDITION

Remote controller operation | Operation condition
Trunk open |

- Vehicle speed is less than 5 km/h (3 MPH)
- Press and hold the trunk open button for 0.5 second or more*
- Ignition switch is except the ON position
- More than 3 seconds are passed since intelligent Key is removed from key slot.
- Panic alarm is not activated.
- Trunk lid opener cancel switch is ON

*: Pattern of trunk open button can be selected using CONSULT-III. Refer to CONSULT-III Function (BCM - INTELLIGENT KEY).
HAZARD AND HORN REMINDER FUNCTION
When doors are locked or unlocked by Intelligent Key, BCM blinks hazard warning lamps as a reminder and transmits horn chirp signal to IPDM E/R. IPDM E/R sounds horn as a reminder.
The hazard and horn reminder has a horn chirp mode (C mode) and a non-horn chirp mode (S mode).
Operating Function of Hazard and Horn Reminder

| C mode | S mode
Intelligent Key operation | Lock | Unlock | Trunk open | Lock | Unlock | Trunk open
Hazard warning lamp blinks | Twice | Once | — | Twice | — | —
Horn sound | Once | — | — | — | — | —

Hazard and horn reminder does not operate in the following condition.

- Ignition switch position is ON
- Door is open (only lock operation)

How to change hazard and horn reminder mode
With CONSULT-III
Refer to CONSULT-III Function (BCM - INTELLIGENT KEY).
Without CONSULT-III
When LOCK and UNLOCK signals are sent from the Intelligent Key for more than 2 seconds at the same time, the hazard and horn reminder mode is changed and hazard warning lamp blinks and horn sounds as per the following items:
AUTO DOOR LOCK FUNCTION
When all doors and fuel lid are locked, ignition switch is OFF (ignition switch is not pressed) and key switch is OFF (Intelligent Key is not inserted in key slot), doors and fuel lid are unlocked with Intelligent Key button. When BCM does not receive the following signals within 60 seconds, all doors and fuel lid are locked.

- Door switch is ON (door is open)
- Door is locked
- Ignition switch is ON
- Key switch is ON (Intelligent Key is inserted in key slot)

Auto door lock mode can be changed by the “AUTO LOCK SET” mode in “WORK SUPPORT”. Refer to CONSULT-III Function (BCM - INTELLIGENT KEY).
PANIC ALARM FUNCTION
When Intelligent Key panic alarm button is pressed, head lamp blinks and horn sounds. For panic alarm function, refer to System Description.
INTERIOR ROOM LAMP CONTROL
Intelligent Key system turns on interior lamp by receiving UNLOCK signal from Intelligent Key. For detailed description, refer to System Description.
LIST OF OPERATION RELATED PARTS
Parts marked with × are the parts related to operation.

Remote keyless entry functions | Intelligent Key | Key slot | Door request switch (Driver, Passenger) | Door switch | Door lock actuator | Intelligent Key warning buzzer | CAN communication system | BCM | Combination meter | Unified meter and A/C amp. | Hazard warning lamp | Horn | IPDM E/R | Trunk lid opener actuator
Door lock/unlock function | × | × |  | × | × |  | × | × |  |  |  |  |  |
Trunk open function | × |  |  |  |  | × | × | × |  | × |  |  |  | ×
Hazard and horn reminder function | × |  |  |  |  | × | × | × | × |  | × | × | × |
Selective unlock function | × |  |  | × | × |  | × | × |  |  |  |  |  |
Auto door lock function | × | × |  | × |  |  | × | × |  |  |  |  |  |