NOTE： Check the tail lamp circuit if the tail lamp and the license plate lamp are not turned ON. 1.CHECK LICENSE PLATE LAMP OPERATION IPDM E/R AUTO ACTIVE TEST

1. Activate IPDM E/R auto active test. Refer to Diagnosis Description.
2. Check that the license plate lamp is turned ON.

CONSULT-III ACTIVE TEST

1. Select "EXTERNAL LAMPS" of IPDM E/R active test item.
2. With operating the test items, check that the license plate lamp is turned ON.

   TAIL | : License plate lamp ON
   Off | : License plate lamp OFF

Is the license plate lamp turned ON?
YES>>License plate lamp circuit is normal.
NO>>Refer to Diagnosis Procedure.