REMOVAL

1.Remove the trunk lid finisher inner. Refer to Removal and Installation.

2.Disconnect the harness connector of trunk lid lock assembly (1) and the harness connectors (A) of high-mounted stop lamp.

3.Remove the mounting nuts (A) of rear wing assembly.

4.Apply protective tape (A) around the outer edge of mating surface between rear wing assembly and trunk lid to prevent from damage.

5.Disengage the clips with the remover tool while peeling the double-faced adhesive tape with threads.
■ CAUTION ■
Never bore the rear wing assembly with excessive power. It may cause cracks in the paint.

6.Replace the following parts after removing the rear wing assembly.

- High-mounted stop lamp: Refer to Removal and Installation.
- Clip and grommet for rear wing assembly
- EPT sealer

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■

- Never disassemble the rear wing assembly.
- Replace the double-faced adhesive tape of the back surface with new tape when reusing the rear wing assembly.

- Remove the double-faced adhesive tape remaining on the rear wing assembly with a double-faced adhesive tape remover.
- Remove any double-faced adhesive tape remaining on the vehicle side in a similar manner, and then apply the primer for painted surfaces (Nissan parts dealer).
- Heat the rear wing assembly application surface and panel surface to 20°C (68 °F) or more.
- Press-fit the entire area of the double-faced adhesive tape with 5 kg/cm2 or more of pressure after applying the rear wing assembly on the vehicle body.

- Replace the EPT sealer of the back surface with new sealer when reusing the rear wing assembly.
  Remove the EPT sealer remaining on the rear wing assembly using a double-faced adhesive tape remover.
- To maintain adhesion, never wash the vehicle within 24 hours after performing the above work.