1.CHECK HEADLAMP (HI) OPERATION IPDM E/R AUTO ACTIVE TEST

1. Activate IPDM E/R auto active test. Refer to Diagnosis Description.
2. Check that the headlamp switches to the high beam.

CONSULT-III ACTIVE TEST

1. Select “EXTERNAL LAMPS” of IPDM E/R active test item.
2. With operating the test items, check that the headlamp (HI) is turned ON.

   Hi | : Headlamp (HI) ON
   Off | : Headlamp (HI) OFF

   NOTE：
   ON/OFF is repeated 1 second each.

Is the headlamp (HI) turned ON/OFF?
YES>>Headlamp (HI) circuit is normal.
NO>>Refer to Diagnosis Procedure.