REMOVAL

1.Remove tires with power tool. Refer to Exploded View.

2.At first, remove the following parts as a set.

- Engine and front final drive: refer to Exploded View (GT-R certified NISSAN dealer).
- Drive shaft: refer to Exploded View (GT-R certified NISSAN dealer).

3.Remove the following parts.

- Steering knuckle and wheel hub and bearing assembly: refer to Exploded View.
- Steering gear assembly and hydraulic line: refer to Exploded View, Exploded View.
- Stabilizer bar and stabilizer connecting rod: refer to Exploded View.
- Transverse link: refer to Exploded View.
- Engine mount insulator: refer to Exploded View (GT-R certified NISSAN dealer).

INSTALLATION
Note the following, and install in the reverse order of removal.

- Perform final tightening of bolts and nuts at the vehicle installation position (rubber bushing), under unladen condition with tires on level ground.