DTC DETECTION LOGIC NOTE：

- If DTC B26E9 is displayed with DTC B2609, first perform the trouble diagnosis for DTC B2609. Refer to DTC Logic.

DTC No. | Trouble diagnosis name | DTC detecting condition | Possible cause
B26E9 | S/L STATUS | BCM requests lock to steering lock unit, then steering lock unit transmits a recognition signal to BCM, but steering lock unit remains unlocked. | Steering lock unit

DTC CONFIRMATION PROCEDURE
1.PERFORM DTC CONFIRMATION PROCEDURE

1. Turn ignition switch ON.
2. Turn ignition switch OFF.
3. Press driver side door switch and wait for at least 1 second.
4. Turn ignition switch ON.
5. Check “Self diagnostic result” with CONSULT-III.

Is DTC detected?
YES>>Refer to Diagnosis Procedure.
NO>>INSPECTION END