DTC DETECTION LOGIC

DTC | Display Item | Malfunction detected condition | Possible causes
C1D17 | BATTERY VOLT | A malfunction is detected in the battery supply voltage to E-SUS control unit. |

- Harness or connector
- E-SUS control unit

DTC REPRODUCTION PROCEDURE
1.DTC REPRODUCTION PROCEDURE
With CONSULT-III

1. Turn the ignition switch OFF to ON.
2. Perform “E-SUS” self-diagnosis.

Is DTC “C1D17” detected?
YES>>Proceed to diagnosis procedure. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END