FUEL PRESSURE RELEASE With CONSULT-III

1.Turn ignition switch ON.

2.Perform “FUEL PRESSURE RELEASE” in “WORK SUPPORT” mode with CONSULT-III.

3.Start engine.

4.After engine stalls, crank it two or three times to release all fuel pressure.

5.Turn ignition switch OFF.

Without CONSULT-III

1.Remove fuel pump fuse (1) located in IPDM E/R (2).

2.Start engine.

3.After engine stalls, crank it two or three times to release all fuel pressure.

4.Turn ignition switch OFF.

5.Reinstall fuel pump fuse after servicing fuel system.

FUEL PRESSURE CHECK
■ CAUTION ■
Before disconnecting fuel line, release fuel pressure from fuel line to eliminate danger.
NOTE：

- Prepare pans or saucers under the disconnected fuel line because the fuel may spill out. The fuel pressure cannot be completely released because R35 models do not have fuel return system.
- Use Fuel Pressure Gauge Kit [SST:(J-44321)] to check fuel pressure.

1.Release fuel pressure to zero.

2.Install the inline fuel quick disconnected fitting (A) between fuel damper (1) and injector tube.

3.Connect the fuel pressure test gauge (quick connector adapter hose) (B) to the inline fuel quick disconnected fitting.

4.Turn ignition switch ON and check for fuel leakage.

5.Start engine and check for fuel leakage.

6.Read the indication of fuel pressure gauge.

At idling | : Approximately 350 kPa (3.57 kg/cm2, 51 psi)

7.If result is unsatisfactory, check fuel hoses and fuel tubes for clogging.If OK, Replace “fuel filter and fuel pump assembly”.If NG, Repair or replace malfunctioning part.