General maintenance includes those items which should be checked during the normal day-to-day operation of the vehicle. They are essential if the vehicle is to continue operating properly. The owners can perform checks and inspections themselves or have a GT-R certified NISSAN dealers do them.
OUTSIDE THE VEHICLE

The maintenance items listed here should be performed from time to time, unless otherwise specified.
Item | Reference page
Tires | Check the pressure with a gauge often and always prior to long distance trips. Adjust the pressure in all tires to the pressure specified. Check carefully for damage, cuts or excessive wear. NOTE：

- Check the pressure of all four tires on the multi function display. See the separate Multi Function Display Owner’s Manual.
- The tires of this vehicle are filled with nitrogen gas. When the tire pressure is low, fill the tires with nitrogen. Contact a GT-R certified NISSAN dealer for information on filling the tires with nitrogen.
- If nitrogen is not available, compressed air may be safely used under normal driving conditions. However, NISSAN recommends refilling with nitrogen for maximum tire performance.

Tire
Wheel nuts | When checking the tires, make sure no nuts are missing, and check for any loose nuts. Tighten if necessary. | —
Tire rotation | Tires cannot be rotated because the vehicle is equipped with different sized tires in the front and rear. | —
Tire Pressure Monitoring System (TPMS) transmitter components | Replace the TPMS transmitter grommet seal, valve core and cap when the tires are replaced due to wear or age. | Exploded View
Tire, wheel alignment and balance | If the vehicle should pull to either side while driving on a straight and level road, or if you detect uneven or abnormal tire wear, there may be a need for wheel alignment. If the steering wheel or seat vibrates at normal highway speeds, wheel balancing may be needed. Wheel alignment needs to be measured and adjusted by a GT-R certified NISSAN dealer.
Tire
Inspection
Inspection
Windshield | Clean the windshield on a regular basis. Check the windshield at least every six months for cracks or other damage. Have a damaged windshield repaired by a qualified repair facility. | —
Windshield wiper blades | Check for cracks or wear if they do not wipe properly. | —
Doors and engine hood | Check that all doors and the engine hood operate properly. Also make sure that all latches lock securely. Lubricate if necessary. Make sure that the secondary latch keeps the hood from opening when the primary latch is released. When driving in areas using road salt or other corrosive materials, check lubrication frequently.
Lubricating
Lamps | Clean the headlamps on a regular basis. Make sure that the headlamps, stop lamps, tail lamps, turn signal lamps, and other lamps are all operating properly and installed securely. Also check headlamp aim. | —

INSIDE THE VEHICLE

The maintenance items listed here should be checked on a regular basis, such as when performing periodic maintenance, cleaning the vehicle, etc.
Item | Reference page
Warning lamps and chimes | Make sure that all warning lamps and chimes are operating properly. | —
Windshield wiper and washer | Check that the wipers and washer operate properly and that the wipers do not streak. | —
Windshield defroster | Check that the air comes out of the defroster outlets properly and in sufficient quantity when operating the heater or air conditioner. | —
Steering wheel | Check that it has the specified play. Check for changes in the steering condition, such as excessive play, hard steering or strange noises. Free play: Less than 35 mm (1.38 in) | —
Seats | Check seat position controls such as seat adjusters, seatback recliner, etc. to make sure they operate smoothly and that all latches lock securely in every position. Check that the head restrains move up and down smoothly and that the locks (if equipped) hold securely in all latched positions.
—
Seat belts | Check that all parts of the seat belt system (e.g. buckles, anchors, adjusters and retractors) operate properly and smoothly, and are installed securely. Check the belt webbing for cuts, fraying, wear or damage. | Inspection
Accelerator pedal | Check the pedal for smooth operation and make sure the pedal does not catch or require uneven effort. Keep the floor mat away from the pedal. | —
Brakes | Check that the brakes do not pull the vehicle to one side when applied. | —
Brake pedal and booster | Check the pedal for smooth operation. If the brake pedal suddenly goes down further than normal, the pedal feels spongy or the vehicle seems to take longer to stop, see a GT-R certified NISSAN dealer immediately. Keep the floor mat away from the pedal.
Inspection and Adjustment
Inspection
Parking brake | Check the parking brake operation regularly. The vehicle should be securely held on a fairly steep hill with only the parking brake applied. If the parking brake needs to be adjusted, see a GT-R certified NISSAN dealer. | Inspection and Adjustment
Transmission "Park" mechanism | On a fairly steep hill, check that the vehicle is held securely with the shift lever in the P (Park) position without applying any brakes. | —

UNDER THE HOOD AND VEHICLE

The maintenance items listed here should be checked periodically (e.g. each time you check the engine oil or refuel).
Item | Reference page
Windshield washer fluid | Check that there is adequate fluid in the reservoir. | —
Engine coolant level | Check the coolant level when the engine is cold. | Inspection
Radiator and hoses | Check the front of the radiator and clean off any dirt, insects, leaves, etc., that may have accumulated. Make sure the hoses have no cracks, deformation, deterioration, rot or loose connections. | —
Brake fluid level | Make sure that the brake fluid level is between the “MAX” and “MIN” lines on the reservoir. | Inspection
Battery | Check the fluid level in each cell. It should be between the “MAX” and “MIN” lines. Vehicles operated in high temperatures or under severe conditions require frequent checks of the battery fluid level. | How to Handle Battery
Engine drive belt | Make sure that no belt is frayed, worn, cracked or oily. | Checking
Engine oil level | Check the level after parking the vehicle on a level spot and turning off the engine. Wait at least 5 minutes for the oil to drain back into the oil pan before checking the oil. | Inspection
Power steering fluid level and lines | Check the level when the fluid is cold, with the engine off. Check the lines for improper attachment, leaks, cracks, etc. | Inspection
Exhaust system | Make sure there are no loose supports, cracks or holes. If the sound of the exhaust seems unusual or there is a smell of exhaust fumes in the engine compartment, immediately have the exhaust system inspected by a GT-R certified NISSAN dealer.
Inspection (GT-R certified NISSAN dealer)
Underbody | The underbody is frequently exposed to corrosive substances such as those used on icy roads or to control dust. It is very important to remove these substances, otherwise rust will form on the floor pan, frame, fuel lines and around the exhaust system. At the end of winter, the underbody should be thoroughly flushed with plain water, being careful to clean those areas where mud and dirt can easily accumulate.
—
Fluid leaks | Check under the vehicle for fuel, oil, water or other fluid leaks after the vehicle has been parked for a while. Water dripping from the air conditioner after use is normal. If you should notice any leaks or gasoline fumes are evident, check for the cause and correct it immediately.
—