INSPECTION AFTER REMOVAL Check components for deformation, cracks and other damage. Replace it if necessary. Ball Joint Inspection Check boots of transverse link, upper link and steering outer socket ball joint for breakage, axial play, and torque. Refer to Inspection (GT-R certified NISSAN dealer), Inspection (GT-R certified NISSAN dealer) and Inspection (GT-R certified NISSAN dealer).
INSPECTION AFTER INSTALLATION

1.Check wheel sensor harness for proper connection. Refer to Exploded View (GT-R certified NISSAN dealer).

2.Check the wheel alignment. Refer to Inspection.

3.Adjust neutral position of steering angle sensor. Refer to Special Repair Requirement (GT-R certified NISSAN dealer).