DTC DETECTION LOGIC

DTC | Self-diagnosis name | DTC detection condition | Possible cause
P2716 | Pressure control solenoid "D" electrical | A DTC is set if the axis B feed pressure solenoid valve monitor current value is less than 0.2 A when the axis B feed pressure solenoid valve target current value is more than 0.38 A. |

- Axis B feed pressure solenoid valve
- Harness or connector
  (Open or short in the axis B feed pressure solenoid valve circuit)

DTC CONFIRMATION PROCEDURE
1.PREPARATION BEFORE OPERATION
If another “DTC CONFIRMATION PROCEDURE” is performed just before the next test, turn the ignition switch OFF and wait for 10 seconds or more, then perform the next test.
>>GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDURE
With CONSULT-III

1. Turn the ignition switch ON.
2. Shift the shift lever to the N position.
   ■ CAUTION ■
   No shift position indicator in the combination meter blinks.
3. Start the engine.
4. With the shift lever in the N position, and run at idle for 5 seconds or more.
5. Check “Self Diagnostic Result” of “TRANSMISSION”.

Without CONSULT-III

1. Turn the ignition switch ON.
2. Shift the shift lever to the N position.
   ■ CAUTION ■
   No shift position indicator in the combination meter blinks.
3. Start the engine.
4. With the shift lever in the N position, and run at idle for 5 seconds or more.
5. Check self-diagnosis.

Is DTC P2716 detected?
YES>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>Go to Intermittent Incident.