1.CHECK SUB FUEL PUMP RELAY

1. Turn ignition switch OFF.
2. Remove sub fuel pump relay.
3. Check the continuity between sub fuel pump relay terminals under the following conditions.

   Terminals | Condition | Continuity
   3 and 5 | 12 V direct current supply between terminals 1 and 2 | Existed
   No supply | Not existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace sub fuel pump relay.