1.CHECK SHIFT SOLENOID VALVE 3 Check the resistance between transmission unit harness connector terminal and ground.

Transmission unit harness connector | Ground | Condition | Resistance (Approx.)
Connector | Terminal
B49 | 27 | Ground | Transmission oil temperature: 20°C (68°F) | 6.6–7.4Ω
Transmission oil temperature: 50°C (122°F) | 7.3–8.3Ω
Transmission oil temperature: 80°C (176°F) | 8.1–9.2Ω

Is the inspection result normal?
YES>>INSPECTION END
NO>>Repair or replace damaged parts.