Perform the hidden welding point repair procedure for arrow view J by lifting up the flange of parcel shelf with rear waist.

1. | Hemming | 2. | Urethane foam |  |
Unit: mm (in) |  |  |  |
| : Vehicle front |  |  |  |
Replacement parts
• | Rear fender assembly (LH) |  |  |  |

| : Vehicle front |  |  |  |

Unit: mm (in) |  |  |  |
| : Vehicle front |  |  |  |

View J: The flange of parcel shelf with rear waist is lifted up.
POINT

- Perform the hemming to the flange of wheelarch after applying the adhesive.
- Apply the sealing to the flange end.
- Refer to Rear Fender Hemming Process.

  1. | Rear wheel well outer | 2. | Rear fender
  3. | Adhesive | 4. | Sealing

  1. | Outer rear wheelhouse
  2. | Rear fender
  3. | Adhesive
  4. | Sealing