1.INSPECTION START Turn ignition switch to START. Are any cylinders ignited? YES>>GO TO 2. NO>> Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
2.CHECK FUEL INJECTOR FUNCTION
With CONSULT-III

1. Start engine.
2. Perform “POWER BALANCE” in “ACTIVE TEST” mode with CONSULT-III.
3. Check that each circuit produces a momentary engine speed drop.

Without CONSULT-III

1. Start engine.
2. Listen to each fuel injector operating sound.

   Clicking sound should be heard.

Is the inspection result normal?
YES>>INSPECTION END
NO>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).