1.CHECK DAYTIME RUNNING LIGHT RELAY EXCITATION COIL SIDE

1. Turn the ignition switch OFF.
2. Remove the daytime running light relay.
3. Check continuity of the daytime running light relay excitation coil side.

   Daytime running light relay | Continuity
   Terminal
   1 | 2 | Existed

Does continuity exist?
YES>>GO TO 2.
NO>>Replace the daytime running light relay.
2.CHECK DAYTIME RUNNING LIGHT RELAY CONTACT SIDE

1. Apply battery voltage to the daytime running light relay between terminals 1 and 2.
2. Check continuity of the daytime running light relay contact side.

   Daytime running light relay | Condition | Continuity
   Terminal | Voltage
   3 | 4 | Apply | Existed
   Not Apply | Not existed
   5 | Apply | Not existed
   Not Apply | Existed

Is the measurement value normal?
YES>> Daytime running light relay is normal.
NO>>Replace the daytime running light relay.