Applied model | VR38DETT
AWD
Transmission model | GR6Z30A
Transmission | Transmission model code number(*1) | JF00A
Operating system | Remote control floor shifter and paddle shifter
Shift position | P | Fixed to output shaft (engine start is possible)
R | Reverse
N | Neutral (engine start is possible)
A | R | 1←→2←→3←→4←→5←→6
Normal | 1←→2←→3←→4←→5←→6
SNOW | 1←→2←→3←→4←→5←→6
M | R | 6M | Fixed to 6th gear | With the under rev protection automatic shift function
5M | Fixed to 5th gear
4M | Fixed to 4th gear
3M | Fixed to 3rd gear
2M | Fixed to 2nd gear
1M | Fixed to 1st gear
Normal | 6M | Fixed to 6th gear | With the over rev and under rev protection automatic shift function
5M | Fixed to 5th gear
4M | Fixed to 4th gear
3M | Fixed to 3rd gear
2M | Fixed to 2nd gear
1M | Fixed to 1st gear
Gear ratio | 1st gear | 4.056
2nd gear | 2.301
3rd gear | 1.595
4th gear | 1.248
5th gear | 1.001
6th gear | 0.796
Reverse | 3.383
Control system | Electronic controls
Function | Self-diagnosis function | With
Fail safe function | With
Synchronizer system | Borg Warner type triple cone synchronizer
Oil pump | Type | External gear pump
Drive type | Drive with the engine
Oil | Recommended | Genuine NISSAN Transmission Oil R35 Special
Capacity | 9.7 liter (10-1/4 US qt, 8-1/2 Imp qt)(*2)

- *1: The model No. refers to the lower five digits of the part number (32000 XXXXX).
- *2: The indicated oil level is only a guide, therefore check the oil level according to the Service Manual.