1.CHECK EVAP CANISTER PURGE VOLUME CONTROL SOLENOID VALVE With CONSULT-III

1. Turn ignition switch OFF.
2. Reconnect all harness connectors disconnected.
3. Disconnect EVAP purge hoses connected to EVAP canister purge volume control solenoid valve.
4. Turn ignition switch ON.
5. Select “PURG VOL CONT/V” in “ACTIVE TEST” mode with CONSULT-III.
6. Touch “Qd” and “Qu” on CONSULT-III screen to adjust “PURG VOL CONT/V” opening and check air passage continuity of EVAP canister purge volume control solenoid valve under the following conditions.

Condition (PURG VOL CONT/V value) | Air passage continuity between (A) and (B)
100% | Existed
0% | Not existed

Without CONSULT-III

1. Turn ignition switch OFF.
2. Disconnect EVAP canister purge volume control solenoid valve harness connector.
3. Disconnect EVAP purge hoses connected to EVAP canister purge volume control solenoid valve.
4. Check air passage continuity of EVAP canister purge volume control solenoid valve under the following conditions.

   Condition | Air passage continuity between (A) and (B)
   12V direct current supply between terminals 1 and 2 | Existed
   No supply | Not existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace EVAP canister purge volume control solenoid valve