1.PERFORM INITIALIZATION Perform initialization with CONSULT-III. Reregister all Intelligent Keys. For initialization and registration of Intelligent Key. Refer to “CONSULT-III Operation Manual NATS-IVIS/NVIS”. Can the system be initialized and can the engine be started with reregistered Intelligent Key?
YES>>INSPECTION END
NO>>GO TO 2.
2.REPLACE BCM

1. Replace BCM. Refer to Removal and Installation.
2. Perform initialization with CONSULT-III. For initialization, refer to “CONSULT-III Operation Manual NATS-IVIS/NVIS”.

Can the system be initialized and can the engine be started with reregistered Intelligent Key?
YES>>INSPECTION END
NO>>GO TO 3.
3.REPLACE ECM

1. Replace ECM. Refer to Special Repair Requirement (GT-R certified NISSAN dealer).
2. Perform initialization with CONSULT-III.

Can the system be initialized and can the engine be started with reregistered Intelligent Key?
YES>>INSPECTION END
NO>>GO TO 4.
4.CHECK INTERMITTENT INCIDENT
Refer to Intermittent Incident.
>>INSPECTION END