REMOVAL

1. | Spacer | 2. | Steering gear assembly | 3. | Cotter pin
4. | Heat insulator |  |  |  |
: Vehicle front
Refer to Components for symbols in the figure.

DISASSEMBLY

1. | Rear cover cap | 2. | Power steering solenoid valve | 3. | Gear-sub assembly
4. | O-ring | 5. | Adjusting screw | 6. | Spring
7. | Retainer | 8. | Gear housing assembly | 9. | Boot clamp (stainless wire)
10. | Spacer | 11. | Inner socket | 12. | Boot
13. | Boot clamp | 14. | Outer socket | 15. | Cylinder tubes
16. | Copper washer |  |  |  |
: Apply power steering fluid.
: Apply Genuine High Performance Thread Sealant or equivalent. Refer to Recommended Chemical Products and Sealants.
: Apply Genuine Medium Strength Thread Locking Sealant or equivalent. Refer to Recommended Chemical Products and Sealants.
: Apply multi-purpose grease.
Refer to Components for symbols not described on the above.