1.CHECK SEAT BELT BUCKLE SWITCH (DRIVER SIDE)

1. Turn ignition switch OFF
2. Disconnect seat belt buckle switch connector.
3. Check continuity of seat belt buckle (driver side).

   Seat belt buckle switch (driver side) | Condition | Continuity
   Terminal
   2 | 3 | When driver side seat belt is not fastened | Existed
   When driver side seat belt is fastened | Not existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace seat belt buckle switch (driver side).