REMOVAL

1.Remove instrument panel (assist). Refer to Exploded View.

2.Remove mounting nuts (A).

3.Disconnect ECM connectors, and then remove ECM (1) with bracket attached.

4.Remove power steering control unit. Refer to Exploded View (GT-R certified NISSAN dealer).

5.Remove mounting screws of intake door motor, and then remove intake door motor from blower unit.

6.Disconnect intake door motor connector.

INSTALLATION
Installation is basically the reverse order of removal.