DETAILED FLOW 1.INTERVIEW FROM THE CUSTOMER Clarify customer complaints before inspection. First of all, reproduce symptoms, and understand them fully. Ask customer about his/her complaints carefully. Check symptoms by driving vehicle with customer, if necessary.
■ CAUTION ■
Customers are not professional. Never guess easily like “maybe the customer means that...,” or “maybe the customer mentions this symptom”.
>>GO TO 2.
2.CHECK AWD WARNING LAMP
Start the engine and drive at 30 km/h (19 MPH) or more for approximately 1 minute.
Does AWD warning lamp turn ON?
YES>>GO TO 3.
NO >>GO TO 6.
3.PERFORM SELF-DIAGNOSIS
With CONSULT-III

1. Perform self-diagnosis for “ALL MODE AWD/4WD”.
2. Check malfunction detected by self-diagnosis.
3. Erase self-diagnostic results for “ALL MODE AWD/4WD”.

>> GO TO 4.
4.CHECK TERMINALS AND HARNESS CONNECTORS
Check pin terminals for damage or loose connection with harness connector.
>>GO TO 5.
5.CHECK SYMPTOM REPRODUCTION
With CONSULT-III
Perform DTC reproduction procedure for the error system.
Is any error detected?
YES>>GO TO 2.
NO >>GO TO 6.
6.PERFORM SYMPTOM DIAGNOSIS
Perform the symptom diagnosis for each system.
Is any malfunction present?
YES>>GO TO 2.
NO >>GO TO 7.
7.FINAL CHECK
With CONSULT-III
Check input/output signal standard of “ALL MODE AWD/4WD”.
Is the input/output the standard value?
YES>>INSPECTION END
NO>>GO TO 2.