REMOVAL ■ CAUTION ■

- Oil filter is provided with relief valve. Use genuine NISSAN oil filter or equivalent.
- Be careful not to get burned when engine and engine oil may be hot.
- When removing, prepare a shop cloth to absorb any engine oil leakage or spillage.
- Never allow engine oil to adhere to drive belt.
- Completely wipe off any engine oil that adheres to engine and vehicle.

1.Remove front undercover. Refer to Exploded View.

2.Using oil filter wrench [SST: KV10115801 (J-38956)] (A), remove oil filter.

| : Vehicle front

INSTALLATION

1.Remove foreign materials adhering to oil filter installation surface.

2.Apply engine oil to the oil seal contact surface of new oil filter.

3.Screw oil filter manually until it touches the installation surface, then tighten it by 2/3 turn (A). Or tighten to the specification.

Oil filter:
| : 17.7 N·m (1.8 kg-m, 13 ft-lb)