REMOVAL ■ CAUTION ■ Never drop or strike front vertical G sensor, or do not use power tool etc., because front vertical G sensor is sensitive to the impact.

1.Turn the ignition switch OFF.

2.Remove the hood ledge cover RH. Refer to Exploded View.

3.Disconnect the front vertical G sensor connector.

4.Remove the front vertical G sensor mounting bolts.

5.Remove the front vertical G sensor.

INSTALLATION
Install in the reverse order of removal.
■ CAUTION ■
Never drop or strike front vertical G sensor, or do not use power tool etc., because front vertical G sensor is sensitive to the impact.