REMOVAL ■ WARNING ■ Be careful not to get burned, as engine oil may be hot.

1.Remove engine undercover. Refer to Exploded View.

2.Remove front undercover. Refer to Exploded View.

3.Remove front bumper. Refer to Exploded View.

4.Remove air duct from oil cooler.

5.Remove air duct bracket.

6.Disconnect oil cooler hoses from oil cooler pipes.
■ CAUTION ■
When oil cooler hoses are disconnected, attach plug to prevent engine oil leakage.

7.Remove oil cooler.
■ CAUTION ■

- Never damage or scratch oil cooler core when removing.
- When oil cooler is removed, attach plug to prevent engine oil leakage.

8.Remove oil cooler pipes if necessary.

INSTALLATION
Note the following, and install in the reverse order of removal.
Oil cooler pipe
If oil cooler pipes are removed, install it as follows:

1.Install oil cooler pipes and pipe bracket, and temporarily tighten the pipe bracket bolt.

2.Temporarily tighten the oil cooler pipe bolts. (oil cooler upper side)

3.Tighten pipe bracket bolt to the specified torque.

4.Tighten oil cooler pipe bolts to the specified torque. (oil cooler upper side)