FAIL-SAFE If the CAN communication with each unit is activates, the combination meter broken the fail-safe control.

System | Processing
Speedometer | Returns to zero when communication is blocked.
Tachometer
Engine coolant temperature gauge
Meter illumination control | Shifts to night mode when communication is blocked.
Shift position indicator | Turned OFF when communication is blocked.
Information display | Door open warning | Indication is turned OFF when communication is blocked.
Trunk open warning
Parking brake release warning
Shift “ P ” warning
Transmission system check
Shift lever position warning
Transmission clutch high temperature warning
Transmission oil high temperature warning
Transmission system warning
Run-flat tire warning
Low tire pressure warning
Tire pressure monitoring system warning
AWD clutch high temperature warning
Front/rear tire size discrepancy warning
AWD system warning
Anti-lock braking system (ABS) warning
Vehicle dynamic control (VDC) system warning
Engine system warning
CRUISE control system warning
CRUISE control system status
Vehicle speed display | 0 km/h (0 MPH) is indicated when communication is blocked.
Possible driving distance | Displays the last calculation result calculated under a normal status when communication is blocked.
Average fuel consumption
Instantaneous fuel consumption
Average vehicle speed
Warning buzzer | Warning is turned OFF when communication is blocked.
Warning lamp/indicator lamp | ABS warning lamp | Turned ON when communication is broken.
VDC OFF warning lamp
SLIP indicator lamp
Brake warning lamp
AWD warning lamp
Malfunction indicator lamp (MIL)
Tire pressure warning lamp | Blinks first, then illuminates after approximately 1 minute.
High beam indicator lamp | Turned OFF when communication is broken.
Turn signal indicator lamp
Tail lamp indicator lamp
CRUISE indicator lamp
SET indicator lamp
KEY warning lamp
Up-shift indicator (green)
Up-shift indicator (yellow)
Up-shift indicator (red)
Transmission check warning lamp