IN-VEHICLE SENSOR

- The in-vehicle sensor (1) is installed to the instrument lower panel (driver).
- The in-vehicle sensor converts the interior air temperature of the passenger room sucked by the aspirator detected with the thermistor into the voltage, and the A/C auto amp. inputs this voltage.

ASPIRATOR
The aspirator (1) generates the vacuum by the air blown from the heater and cooling unit and draws the air of the passenger room to the in-vehicle sensor area via the aspirator duct.

| : Vehicle front

INTERIOR AIR TEMPERATURE CORRECTION

- The A/C auto amp. inputs the temperature detected with the in-vehicle sensor as the interior air temperature.
- Perform the correction of the temperature detected with the in-vehicle sensor for each air conditioner control.