1.CHECK FUEL PUMP CONTROL MODULE (FPCM)

1. Check the voltage between FPCM terminals under the following conditions.

   FPCM | Condition | Voltage
   Connector | + | −
   Terminal | Terminal
   B230 | 7 | 6 | For 1 second after turning ignition switch ON | Approx. 8.5 V
   More than 1 second after turning ignition switch ON | Approx. 0 V
   Idle speed | Approx. 8.5 V

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace FPCM.