1.PERFORM SELF-DIAGNOSIS With CONSULT-III

1. Turn the ignition switch ON and wait for 2 seconds or more.
2. Perform the “SELF-DIAGNOSIS”.
3. Check if any DTC is detected in the self-diagnostic results.

Is DTC “U1000” displayed?
YES>>Perform the diagnosis for the CAN communication system. Refer to Trouble Diagnosis Flow Chart.
NO>>Perform the intermittent malfunction diagnosis. Refer to Intermittent Incident.