1.REGISTER THE TRANSMITTER ID Perform transmitter ID registration for all wheels. Refer to Transmitter ID Registration Procedure. Is ID registration for all wheels been completed? YES>>GO TO 2. NO>>Change the work location and perform ID registration again, then perform trouble diagnosis. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
2.CHECK TIRE PRESSURE SIGNAL
With CONSULT-III

1. Drive for 3 minutes at a speed of 40 km/h (25 MPH) or more, then drive normally for 10 minutes.
2. Within 5 minutes, select “DATA MONITOR” for the CONSULT-III “AIR PRESSURE MONITOR”.
3. Display the following: “AIR PRESS FL”, “AIR PRESS FR”, “AIR PRESS RR”, and “AIR PRESS RL”.
4. Check that the tire pressures is the specified value.

   Monitor item | Condition | Displayed value
   AIR PRESS FL | Drive for 3 minutes at a speed of 40 km/h (25MPH) or more, then drive normally for 10 minutes. | Internal pressure of tires
   AIR PRESS FR
   AIR PRESS RR
   AIR PRESS RL

Is the inspection result normal?
YES>>GO TO 3.
NO>>Change the work location, then GO TO 1.
3.CHECK THE DIAGNOSIS RESULTS
With CONSULT-III

1. Erase the self-diagnosis memory of the low tire pressure warning control unit.
2. Turn ignition switch OFF, and wait for 10 seconds or more.
3. Perform self-diagnosis of the low tire pressure warning control unit.

Are DTC “C1755”, “C1756”, “C1757”, or “C1758” and “C1708”, “C1709”, “C1710”, or “C1711” detected?
YES>>Change the work location, then GO TO 1.
NO>>GO TO 4.
4.CHECK TIRE PRESSURE SIGNAL
With CONSULT-III

1. Drive for 3 minutes at a speed of 40 km/h (25 MPH) or more, then drive normally for 10 minutes.
2. Within 5 minutes, select “DATA MONITOR” for the CONSULT-III “AIR PRESSURE MONITOR”.
3. Display the following: “AIR PRESS FL”, “AIR PRESS FR”, “AIR PRESS RR”, and “AIR PRESS RL”.
4. Check that the tire pressures is the specified value.

   Monitor item | Condition | Displayed value
   AIR PRESS FL | Drive for 3 minutes at a speed of 40 km/h (25MPH) or more, then drive normally for 10 minutes. | Internal pressure of tires
   AIR PRESS FR
   AIR PRESS RR
   AIR PRESS RL

Is the inspection result normal?
YES>>INSPECTION END
NO>>Change the work location, then GO TO 1.