■ CAUTION ■ Before performing the diagnosis, check that the following is normal.

- Interior room lamp power supply
- Trunk room lamp bulb

1.CHECK TRUNK ROOM LAMP OPERATION
CONSULT-III ACTIVE TEST

1. Turn the ignition switch ON.
2. Select “LUGGAGE LAMP TEST” of BCM (INT LAMP) active test item.
3. With operating the test items, check that trunk room lamp operation.

   On | : Trunk room lamp ON
   Off | : Trunk room lamp OFF

Is the trunk room lamp turned ON/OFF?
YES>>Trunk room lamp circuit is normal.
NO>>Refer to Diagnosis Procedure.