■ CAUTION ■ Before replacing BCM, perform “READ CONFIGURATION” to save or print current vehicle specification. Refer to Description. REMOVAL

1.Remove dash side finisher (passenger side). Refer to Exploded View.

2.Remove bolt and nut.

3.Remove BCM and disconnect the connector.

INSTALLATION
Install in the reverse order of removal.
■ CAUTION ■

- Be sure to perform “WRITE CONFIGURATION” when replacing BCM.
- Be sure to perform the system initialization (NATS) when replacing BCM. Refer to Work Procedure.