DTC DETECTION LOGIC

DTC | Display contents of CONSULT-III | Diagnostic item is detected if ... | Probable malfunction location
B2321 | OIL LEV SEN OPEN | Oil level sensor signal circuit is open. (Resistance value of oil level sensor exceeds 20 Ω) |

- Oil level sensor signal circuit
- Oil level sensor

B2322 | OIL LEV SEN SHORT | Oil level sensor signal circuit is shorted. (Resistance value of oil level sensor is less than 3 Ω)

NOTE：
When the following conditions are satisfied, the combination meter reads the resistance value of oil level sensor. The combination meter does not read the oil level sensor resistance value within 5 minutes after the previous reading of oil level sensor resistance value by the combination meter.

1. Turn the ignition switch OFF.
2. Wait for 5 minutes or more, then open the driver door.

DTC (B2321: OIL LEV SEN OPEN, B2322: OIL LEV SEN SHORT) is also detected at the timing described above.