INSPECTION AFTER REMOVAL

- Check that the muffler finisher installation position, referring to the figure.

  A | : Under view
  B | : Protrusion (main muffler assembly side)
  c | : 28 mm (1.10 in)
  | : Vehicle front

  ■ CAUTION ■
  Be sure to correct the installation position if it is different from the position shown in the figure.

INSPECTION AFTER INSTALLATION

- Check that clearance between muffler finisher and rear bumper is even.

- If the clearance is not even, reinstall main muffler assembly.
  ■ CAUTION ■
  When reinstalling main muffler assembly, check the muffler finisher installation position. Refer to “INSPECTION AFTER REMOVAL”.

- With engine running, check exhaust tube joints for gas leakage and unusual noise.
- Check to ensure that mounting brackets are installed properly and free from undue stress. Improper installation may result in excessive noise and vibration.