1.PERFORM ACTIVE TEST With CONSULT-III

1. Connect the E-SUS control unit harness connector.
2. Connect the set-up switch (suspension) connector.
3. Select “MODE LAMP” in “ACTIVE TEST”.
4. On the display, touch “ON” or “OFF”, and check that the system operates as shown in the table below.

Test item | Display Item | Display Item
Illumination status
ON | OFF
MODE LAMP | R | ON | OFF
COMF

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace the set-up switch (suspension).