1.CHECK OPERATION

1. Press the AUTO switch, and then check that “AUTO” is shown on the display.
2. Operate the temperature control dial (driver side). Check that the fan speed or discharge air changes (the discharge air temperature or fan speed varies depending on the ambient temperature, in-vehicle temperature, and set temperature).

Does it operate normally?
YES>>INSPECTION END
NO>>Perform the diagnosis for the A/C auto amp. Refer to Diagnosis Procedure.