1.CHECK MANIFOLD ABSOLUTE PRESSURE (MAP) SENSOR

1. Turn ignition switch OFF.
2. Remove MAP sensor with its harness connector.
3. Install pressure pump (A) to MAP sensor (1).
4. Turn ignition switch ON.
5. Check the voltage between ECM harness connector terminals under the following conditions.
   NOTE：
   - Always calibrate the pressure pump gauge when using it.
   - Inspection should be done at room temperature [10 - 30°C (50 - 86°F)].

   ECM | Condition [Pressure (Relative to atmospheric pressure)] | Voltage
   Connector | + | −
   Terminal | Terminal
   F101 | 48 [MAP sensor] | 74 | 0 kPa (0 mmHg, 0 inHg) | Approx. 2.03 V
   +40 kPa (300 mmHg, 11.81 inHg) | Approx. 2.67 V

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace MAP sensor.