Item | Function
BCM | Controls the door lock function.
Door lock and unlock switch | Inputs lock or unlock signal to BCM.
Door lock actuator | Inputs lock/unlock signal from BCM and locks/unlocks each door.
Door switch | Inputs door open/close condition to BCM.
Key slot | Inputs key insert/remove signal to BCM.
Combination meter | Transmits vehicle speed signal to BCM via CAN communication line.
TCM | Transmits shift position signal to BCM via CAN communication line.
Fuel lid lock actuator | Performs lock/unlock of the fuel lid.
Push-button ignition switch | Input push-button ignition switch ON/OFF condition to BCM.