The underside of the floor and wheelhouse are undercoated to prevent rust, vibration, noise and stone chipping. Therefore, when such a panel is replaced or repaired, apply undercoating to that part. Use an undercoating which is rust resistant, soundproof, vibration-proof, shock-resistant, adhesive, and durable.
Precautions in Undercoating

1.Never apply undercoating to any place unless specified (such as the areas above the muffler and three way catalyst that are subjected to heat).

2.Never undercoat the exhaust pipe or other parts that become hot.

3.Never undercoat rotating parts.

4.Apply bitumen wax after applying undercoating.

5.After putting seal on the vehicle, put undercoating on it.

| : Undercoated areas |  |  |  |
| : Sealed portions |  |  |  |