REMOVAL

1.Remove the hood lock. Refer to Removal and Installation (GT-R certified NISSAN dealer).

2.Remove the fender protector RH. Refer to Removal and Installation.

3.Remove the hood lock control cable clamp of hood ledge.

4.Remove the hood lock control cable protector from hood lock cable clamp of front fender bracket.

5.Remove the hood lock control cable protector cover (rear) from the hood lock control cable protector.

6.Remove the hood lock control cable (rear) from the hood lock control cable protector.

7.Remove the hood lock opener handle mounting bolts from the bottom of lower instrument panel LH, and then remove the hood lock opener handle.

8.Remove the hood lock control cable (rear) from the hood lock opener.

9.Remove the kicking plate inner and the dashboard side lower finisher. Refer to Exploded View.

10.Remove the lower dashboard grommet, and then pull out the hood lock control cable (rear) to outside of passenger room.
■ CAUTION ■
While pulling, never damage (peeling) the outside of the hood lock control cable.

INSTALLATION
Install in the reverse order of removal.
■ CAUTION ■

- Pass the hood lock cable through the opening while keeping the winding radius larger.
- Securely push the grommet into the panel hole.
- Check hood lock control cable is properly engaged with hood lock.
- Check cable is not offset from the positioning grommet, and apply the sealant to the grommet (A) properly.
- After installation, perform the inspection. Refer to Inspection (GT-R certified NISSAN dealer).
- After installation, perform the fitting adjustment. Refer to Adjustment.