NOTE： Check the tail lamp circuit if the tail lamp and the rear side marker lamp are not turned ON. 1.CHECK REAR SIDE MARKER LAMP OPERATION IPDM E/R AUTO ACTIVE TEST

1. Activate IPDM E/R auto active test. Refer to Diagnosis Description.
2. Check that the rear side marker lamp is turned ON.

CONSULT-III ACTIVE TEST

1. Select "EXTERNAL LAMPS" of IPDM E/R active test item.
2. With operating the test items, check that the rear side marker lamp is turned ON.

   TAIL | : Rear side marker lamp ON
   Off | : Rear side marker lamp OFF

Is the rear side marker lamp turned ON/OFF?
YES>>Rear side marker lamp circuit is normal.
NO>>Refer to Diagnosis Procedure.