DTC DETECTION LOGIC

DTC | Display item | Malfunction detected condition | Possible cause
C1115 | ABS SENSOR [ABNORMAL SIGNAL] | When wheel sensor input signal is malfunctioning. |

- Harness or connector
- Wheel sensor
- ABS actuator and electric unit (control unit)

DTC CONFIRMATION PROCEDURE
1.DTC REPRODUCTION PROCEDURE

1. Start the engine and drive the vehicle at 30 km/h (19 MPH) or more for approximately 1 minute.
2. Perform self-diagnosis for “ABS” with CONSULT-III.

Is DTC “C1115” detected?
YES>>Proceed to diagnosis. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END