1.CHECK PASSENGER SIDE POWER WINDOW MOTOR POWER SUPPLY AND GROUND CIRCUIT Check passenger side power window motor power supply and ground circuit. Refer to Diagnosis Procedure. Is the inspection result normal? YES>>GO TO 2.
NO>>Repair or replace the malfunctioning parts.
2.CHECK PASSENGER SIDE POWER WINDOW MOTOR
Check passenger side power window motor.
Refer to Component Function Check .
Is the inspection result normal?
YES>>GO TO 3.
NO>>Repair or replace the malfunctioning parts.
3.CONFIRM THE OPERATION
Confirm the operation again.
Is the inspection result normal?
YES>>Check intermittent incident. Refer to Intermittent Incident.
NO>>GO TO 1.