Diagnostic test mode | Function | ENGINE | TRANSMISSION | ALL MODE AWD/4WD | ABS | AIR BAG | IPDM E/R | BCM | MULTI AV | METER/M&A | E-SUS | AIR PRESSURE MONITOR | HVAC
Work Support | This mode enables a technician to adjust some devices faster and more accurately. | x | x | - | x | - | - | x | x | - | - | x | x
Self Diagnostic Results | Retrieve DTC from ECU and display diagnostic items. | x | x | x | x | x | x | x | x | x | x | x | x
Data Monitor | Monitor the input/output signal of the control unit in real time. | x | x | x | x | - | x | x | x | x | x | x | x
CAN Diagnosis | This mode displays a network diagnosis result about CAN by a diagram. | x | x | x | x | x | x | x | x | x | x | x | x
CAN Diagnosis Support Monitor | It monitors the status of CAN communication. | x | x | x | x | - | x | x | x | x | x | x | x
Active Test | Send the drive signal from CONSULT-III to the actuator. The operation check can be performed. | x | x | x | x | - | x | x | - | - | x | x | x
DTC & SRT confirmation | The status of system monitoring tests and the self-diagnosis status/result can be confirmed. | x | - | - | - | - | - | - | - | - | - | - | -
ECU Identification | Display the ECU identification number (part number etc.) of the selected system. | x | x | x | x | x | x | x | x | - | x | x | x
Function Test | This mode can show results of self-diagnosis of ECU with either “OK” or “NG”. For engine, more practical tests regarding sensors/switches and/or actuators are available. | x | - | - | x | x | - | - | - | - | - | - | -
Configuration | Function to READ/WRITE vehicle configuration. | - | x | - | - | - | - | x | x | - | - | - | -
Special Function | Other results or histories, etc. that are recorded in ECU are displayed. | - | - | - | - | x | - | - | - | x | - | - | -
x: Applicable
*1: If GST application is equipped, functions in accordance with SAE J1979 and ISO 15031-5 can be used.