### System Outline

Door lock control (Lock and unlock) is performed by remote control, without the ignition key inserted in the door key cylinder, using lowpower electrical waves emitted by a transmitter.

1.Normal Operation

*Lock operation
When the lock button on the transmitter is pressed, all the doors are locked.

*Unlock operation
When the unlock button on the transmitter is pressed, all the doors are unlocked.

2.Visual Confirmation of Lock or Unlock

If all doors indicate that they are locked after the lock command, hazard lights will flash once. If any door indicates that it is open after the unlock command, hazard lights will flash twice.

3.Automatic Lock Operation

All the doors are automatically relocked unless any door is opened within 30 seconds after pushing the button (Transmitter) to unlock all the doors under conditions that the ignition key is not inserted into the ignition key cylinder (Unlock warning SW off), ignition SW is at OFF and all the doors are completely closed.