### System Outline

With the ignition SW turned on, the current flows to TERMINAL (B) 2 (LHD) or (B) 3 (RHD) of the front wiper and washer SW, TERMINAL 1 of the windshield washer motor and TERMINAL 2 of the windshield wiper motor through the WIP fuse.

1.Low Speed Position

With the front wiper SW turned to LO position, the current flows from TERMINAL (B) 2 (LHD) or (B) 3 (RHD) of the front wiper and washer SW to TERMINAL (B) 3 (LHD) or (B) 2 (RHD) to TERMINAL 1 (LHD) or 5 (RHD) of the windshield wiper motor to TERMINAL 5 (LHD) or 4 (RHD) to GROUND and causes the windshield wiper motor to run at low speed.

2.High Speed Position

With the front wiper SW turned to HI position, the current flows from TERMINAL (B) 2 (LHD) or (B) 3 (RHD) of the front wiper and washer SW to TERMINAL (B) 4 (LHD) or (B) 1 (RHD) to TERMINAL 4 (LHD) or 3 (RHD) of the windshield wiper motor to TERMINAL 5 (LHD) or 4 (RHD) to GROUND and causes the windshield wiper motor to run at high speed.

3.INT Position

With the front wiper SW turned to INT position, the wiper relay operates and current flows from TERMINAL (B) 2 (LHD) or (B) 3 (RHD) of the front wiper and washer SW to TERMINAL (A) 2 to GROUND. This activates the intermittent circuit and the current flows from TERMINAL (B) 2 (LHD) or (B) 3 (RHD) of the front wiper and washer SW to TERMINAL (B) 3 (LHD) or (B) 2 (RHD) to TERMINAL 1 (LHD) or 5 (RHD) of the windshield wiper motor to TERMINAL 5 (LHD) or 4 (RHD) to GROUND and the wiper operates.
The intermittent operation is controlled by the charge/discharge function of the condenser installed in the relay, and the intermittent time is controlled by a time control SW to change the charging time of the condenser (w/ INT time SW).
Intermittent operation is controlled by a condenser charge and discharge function in the relay (w/o INT time SW).

4.Mist Position

With the front wiper SW turned to MIST position, the current flows from TERMINAL (B) 2 (LHD) or (B) 3 (RHD) of the front wiper and washer SW to TERMINAL (B) 3 (LHD) or (B) 2 (RHD) to TERMINAL 1 (LHD) or 5 (RHD) of the windshield wiper motor to TERMINAL 5 (LHD) or 4 (RHD) to GROUND and causes the windshield wiper motor to run at low speed.

5.Washer Interlocking Operation

With the washer SW pulled to ON position, the current flows from the WIP fuse to TERMINAL 1 of the windshield washer motor to TERMINAL 2 to TERMINAL (A) 3 (LHD) or (A) 1 (RHD) of the front wiper and washer SW to TERMINAL (A) 2 to GROUND and causes the windshield washer motor to run and the window washer to spray. Simultaneously, current flows from the WIP fuse to TERMINAL (B) 2 (LHD) or (B) 3 (RHD) of the front wiper and washer SW to TERMINAL (B) 3 (LHD) or (B) 2 (RHD) to TERMINAL 1 (LHD) or 5 (RHD) of the windshield wiper motor to TERMINAL 5 (LHD) or 4 (RHD) to GROUND, causing the wiper to function.