GSIC - Global Service Information Center

# HEATED OXYGEN SENSOR (for Unleaded Gasoline Specification Vehicle) > INSTALLATION

## for Preparation Click here

1. INSTALL HEATED OXYGEN SENSOR (2WD)

1. Using SST, install the sensor.

   SST
     09224-00010

   Torque:
     44 N*m{ 449 kgf*cm , 32 ft.*lbf }

   Torque:
     40 N*m{ 408 kgf*cm , 30 ft.*lbf } for use with SST

   HINT:
     Use a torque wrench with a fulcrum length of 30 cm (11.81 in.).

1. Connect the sensor connector.

2. INSTALL HEATED OXYGEN SENSOR (4WD)

1. Using SST, install the sensor.

   SST
     09224-00010

   Torque:
     44 N*m{ 449 kgf*cm , 32 ft.*lbf }

   Torque:
     40 N*m{ 408 kgf*cm , 30 ft.*lbf } for use with SST

   HINT:
     Use a torque wrench with a fulcrum length of 30 cm (11.81 in.).

1. Attach the 3 wire clamps to the vehicle body.

1. Connect the sensor connector.

3. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

4. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   CAUTION:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.